{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N8"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B8","RXTP35N2V1B8"]
["Lydtryk","Varme","","Nom.","dBA","49","49"]
["","Køle","","Nom.","dBA","48","48"]
["Standardtilbehør","Installationsvejledning","","","","1","1"]
["","Mærkat for kølemiddelmængde","","","","1","1"]
["","Flersproget mærkat for fluorholdige drivhusgasser","","","","1","1"]
["Kølemiddel","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Opladning","","","kg","1.1","1.1"]
["","Type","","","","R-32","R-32"]
["Blæsermotor","Hastighed","Køle","Super lav","o/min","450","450"]
["","","Varme","Super lav","o/min","360","360"]
["Rørføringsforbindelser","Niveauforskel","IU - OU","Max.","m","15","15"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Mål","Unit","","Width","mm","763","763"]
["","","","Depth","mm","312","312"]
["","","","Height","mm","551","551"]
["Vægt","Unit","","","kg","38","38"]
["Power supply","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","220-240","220-240"]
["Bemærkninger","","","","","(1) - Indeholder drivhusgasser med tilsat fluor","(1) - Indeholder drivhusgasser med tilsat fluor"]
["","","","","","(2) - Se separat tegning for driftsområde","(2) - Se separat tegning for driftsområde"]
["","","","","","(3) - Se særskilte tegninger med de elektriske data","(3) - Se særskilte tegninger med de elektriske data"]